References

**Comment [b30]:** Font size 16; Bold; Center Aligned

1. ACI Committee 229. (1994). “Controlled low-strength materials (CLSM), ACI 229R-94.”Concrete International, 16(7), 55-64.

**Comment [b31]:** Font 12; justified

1. BASF (1990). “Guidelines for use of EPS board products in building construction”, *Technical Bulletin E-I*, Parsippany, N J, USA.
2. Chandra S. and Choudhary R. (2013). “Performance characteristics of bituminous concrete with industrial wastes as filler*”, Journal of Materials in Civil Engineering,* ASCE, 25(11), 1666-1673.
3. Cheung T., Jansen D. C. and Hanson J. L. (2008). “Engineering controlled low strength materials using scrap tire rubber”, *Geo Congress 2008: Characterization, Monitoring and Modelling of Geosystems,* ASCE,622-629.
4. Edeh J. E., Joel M. and Okpe A. (2013). “Laboratory evaluation of reclaimed asphalt pavement–quarry waste blends as unbound highway pavement material”, *Journal of Advances in Civil Engineering Materials,* ASTM, 2(1), 110-120.
5. Gemperline C. S. and Durham S. (2013). “Beneficial use of recycled materials in controlled low strength materials*”, Proceedings of International Conference on Pipelines and Trenchless Technology,* China, ICPTT, 1305-1316.
6. Horvath J. S. (1994). “Expanded polysterene geofoam: an introduction to material behaviour”, *Geotextiles and Geomembranes*, 13, 263-280.
7. IS 2720 (Part 3)-1980. “Indian standard methods of test for soil part 3; Determination of specific gravity”, *Bureau of Indian Standards,* New Delhi, India.